Product Specifications
LeeBoy 8530 Paver 

The following specifications are based on the 8530 Asphalt Paver manufactured by LeeBoy.  Because of continuous equipment research and development, we reserve the right to change these specifications.  For more information, questions or assistance preparing specifications, please contact your local LeeBoy Dealer.

	1.     Dimensions
a. Length: 15’
b. Width:  8’ 6” transport
10’ hopper wings down 
c. Height:  6’ 8” low deck
               7’ 9” high deck
d. Total Weight (with screed):  22,520 lbs.


2. Engine: 
a. Kubota turbocharged diesel
b. Tier 4 Final - 125 HP (93.2 kW)
c. Remote mounted DOC + DPF + SCR
d. MURR I/O distributor blocks with LED lighting


3. Capacities:  
a. Fuel: 32 gallons
b. Hydraulic: 25 gallons
c. Washdown tank: 7 gallons
d. DEF tank:  5 gallons


4. Hopper:
a. Hopper size:  9 ton
b. Hopper height:  31.75”
c. Hopper wings:  Heavy-duty .5” with large radius corners
d. Rear hopper wing wipers


5. Paving Widths:
a. Machine has variable paving widths up to 15’ 6” 


6. Paving Depths:
a. Electronically operated tow point cylinders 
b. Includes manual flights screws positioned on the screed
c. Depth:  0 to 8”


7. Available Screeds:
a. Legend HD PRO Screed: Variable up to 15’6”, weight 4,150 lbs
View detailed Screed specifications



8. Under Auger Material Cutoff:
a. Two independent hydraulically operated 4' wide gates located under the augers and constructed of .375" A-36 plate steel
b. Can be configured to automatically close in reverse
c. Operational from the main control panel or screed controls


9. Material Augers:
a. Two independent, hydraulically driven, segmented augers.  Operated automatically or manually
b. Augers are reversible
c. Variable speed from 0-173 rpm
d. Quick change auger assemblies
e. Augers are 12” diameter, 12” pitch and are cast from .75” HRC 55-60
f. System has manual override functions and automatic functions are controlled by sonic sensors (non-contacting)
g. Single point lube system


10. Conveyors
a. Two independent, hydraulically driven conveyors with automatic shut-off
b. Dual 36” feeding conveyors
c. Conveyors are reversible
d. Front heavy-duty conveyor chain adjustments, does not require lifting of conveyor floor
e. Quad bearings, front and rear conveyor
f. Conveyor is hydraulically raiseable to allow cleaning and service
g. System has manual override functions and automatic functions are controlled by a paddle and proximity sensor. 
h. 3,000 hour Wide-Conveyor Floor Assembly Warranty


11. Operators Platform
a. Includes both right and left hand seats 6’ 1" above ground with a lockable cover for the instrument panel
b. Various pivoting and adjustable swing out seat positions


12. Operators Controls:
a. High deck/low deck configuration
b. Includes dual electronic steer
c. Dual, independent adjustable control stations interchangeable in the field
d. Dash panel includes augers, screed extension, cut-offs, screed, hopper wings, conveyors, grade controls, steering and lights
e. User-friendly, icon-based CAN Bus controls
f. Backlit keypad with LED indicator lights
g. Colored LED, sunlight viewable control screen with digital readouts. Review and monitor system vitals including: RPM, paving speeds, system pressures, screed temperature and generator usage


13. Screed Controls:
a. Screed control boxes are on each side and contain extensions, cutoffs, auger, tow, horn, e-stop and slope


14. Steering:
a. Dual electronic steering controls
b. Machine can be controlled from a high deck position or lowered to control at the screed
c. Electronically controlled pumps operate the forward/reverse motion from dual joysticks


15. Washdown System:
a. Electric HD pump with two 25’ x .375” diameter hose reels and spray nozzles
b. Built in pressure sensor and shutoff
c. Citrus tank sight gauge


16. Hydraulic System:
a. Variable volume hydraulic pumps for each drive
b. Independent constant volume pumps for augers, conveyors, cylinders and charge 
c. Hydraulic oil: all weather, all temperature
d. Dual 77,000 BTU oil coolers


17. Push Rollers:
a. Two 3" diameter rollers with sealed bearings mounted on a swivel frame
b. Vertically adjustable push rollers, 7” of height adjustment
c. Adjustable height push rollers with self-cleaning scrapers


18.  Track Drive System:
a. Hydrostatically powered, self-cleaning crawler type tracks consisting of drive sprocket, seven rollers and hydraulically adjustable front idler
b. Drive mechanism is torque hub driven which consist of two speeds and obtained by means of a keypad button
c. Fail safe brakes
d. Track size:  14” wide x 87” long poly 7 rollers
OR
Rubber Track Option: 15.75” wide x 87” long rubber 7 rollers
e. Paving speed: 0 to 150’ per minute (1.7 mph)
f. Travel speed: 0 to 300’ per minute (3.4 mph)


19. Additional Standard Equipment:
a. Automatic Temperature Control (ATC) Standard
b. Gauge package (oil pressure, hour meter, fuel gauge, volt meter, water temp, tachometer, hydraulic oil temp, engine diagnostics)
c. Actuator-driven hood lift
d. Ground-level service access doors
e. Integrated dual tool boxes on screed
f. Heated end gates
g. Back-up alarm
h. Quick-folding LED beacon light
i. Sliding LED work light package
j. Vandalism protection covers
k. Horn
l. 2 seats
m. USB port
n. Magnetic cup holders


20. Optional Equipment:
a. Additional control post and wire harness, left side
b. Rubber track, continuous
c. Truck hitch
d. Hydraulically extendable oscillating push rollers
e. Steering knob drive controls, in lieu of joysticks
f. Wiring only, grade controls (Topcon)
g. Dual grade control (Topcon)
h. Dual grade and slope (Topcon)
i. LED blade light system, DC powered, 2 individually mounted LED blades
j. Wireless screed remote controls
k. Umbrella mounts (x2)


21. Training, Support and Company:
a. Training and support manuals
b. Optional on-site operator training by Dealer
c. Two-year, unlimited hours warranty against any manufacturer defects
d. Extended warranty available
e. 60+ years manufacturing experience
f. ISO 9001 Certified
g. Sourcewell Contract #060122-VTL
h. Manufactured in USA
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